//Verison=1.0
//Example,Don't Delete flowing text 
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '61 00 02 00 19 00' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//
Send	Command: 84 A9 61 00 02 40 00 00
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-54
Send	Command: 84 A9 61 00 02 40 6C 40
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-1
Send	Command: 84 A9 61 00 02 40 02 5D
Receive	Command:84 A9 61 00 02 40 17 00
PAUSE 100
Command ID:	WMM-2
Send	Command: 84 A9 61 00 02 40 04 15
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-3
Send	Command: 84 A9 61 00 02 40 06 ED
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-4
Send	Command: 84 A9 61 00 02 40 09 18
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-5
Send	Command: 84 A9 61 00 02 40 0A 00
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-6
Send	Command: 84 A9 61 00 02 40 0C 4D
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-7
Send	Command: 84 A9 61 00 02 40 0E 04
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-14
Send	Command: 84 A9 61 00 02 40 1C 00
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-44
Send	Command: 84 A9 61 00 02 40 58 04
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-45
Send	Command: 84 A9 61 00 02 40 5A 10
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-50
Send	Command: 84 A9 61 00 02 40 64 01
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WMM-56
Send	Command: 84 A9 61 00 02 40 70 01
Receive	Command:84 A9 61 00 02 40 17 00
PAUSE 100
Command ID:	WMM-54-STEP3
Send	Command: 84 A9 61 00 02 40 6C 39
Receive	Command:84 A9 61 00 02 40 17 00
