//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
.Set READY_VAR = 01

Command ID:	DMR_CC
Send	Command: 84 A9 61 00 02 05 77 0d
Receive	Data:84 A9 61 00 02 05 77 00
Command ID:	DMR_FLC
Send	Command: 84 A9 61 00 04 05 76 00 00 00
Receive	Data:84 A9 61 00 02 05 76 00
//Command ID:	DMR_CALL_OPTION for 3918 controlled RF
//Send	Command: 84 A9 61 00 06 05 79 c1 00 00 00 00 
Command ID:	DMR_CALL_OPTION
Send	Command: 84 A9 61 00 06 05 79 81 00 00 00 00 
Receive	Data:84 A9 61 00 02 05 79 00
Pause 1000
Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	PROCESS_MODE
Send	Command: 84 A9 61 00 02 00 1A 03
Receive	Data:84 A9 61 00 02 00 1A 00

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 05 7d  01 23 45 67
Receive Data: 84 A9 61 00 02 05 7d 00
Command ID:	OWNID_BCD
Send	Command: 84 A9 61 00 05 05 7e 01 23 45 67 
Receive	Data:84 A9 61 00 02 05 7e 00

Command ID:	REPORT_FIELD
Send	Command: 84 A9 61 00 02 00 1D ff
Receive	Command:84 A9 61 00 02 00 1D 00
Command ID:	DEMOD_GAIN
Send	Command: 84 A9 61 00 03 00 1C 00 00
Receive	Command:84 A9 61 00 02 00 1C 00

Command ID: ALOOP_CODEC_LOOP
Send command: 84 A9 61 00 04 00 18 03 01 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: ALOOP_DECIMATOR_LOOP
Send command: 84 A9 61 00 04 00 18 03 02 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: ALOOP_VOCODER_LOOP
Send command: 84 A9 61 00 04 00 18 03 13 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: ALOOP_PACKET_LOOP
Send command: 84 A9 61 00 04 00 18 03 05 00
Receive Data: 84 A9 61 00 02 00 18 00

Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
//Send	Command: 84 A9 61 00 04 05 78 7f 5d d5
Receive	Data:84 A9 61 00 02 05 78 00
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d1
//Receive	Data:84 A9 61 00 02 30 77 0D
//Receive	Data:84 A9 61 00 04 30 76 7f 5d d5
Receive	Data:84 A9 61 00 04 30 76 00 00 00
Receive	Data:84 A9 61 00 04 30 50 12 D6 87
Receive	Data:84 A9 61 00 04 30 51 12 D6 87
Receive	Data:84 A9 61 00 05 30 7d 01 23 45 67
Receive	Data:84 A9 61 00 05 30 7e 01 23 45 67
Receive	Data:84 A9 61 00 02 30 27 00
pause 1500
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Pause 2000
Command ID: ALOOP_4FSK_LOOP
Send command: 84 A9 61 00 04 00 18 03 06 00
Receive Data: 84 A9 61 00 02 00 18 00



Command ID:	DMR_CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00

Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
//Send	Command: 84 A9 61 00 04 05 78 7f 5d d5
Receive	Data:84 A9 61 00 02 05 78 00
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d1
//Receive	Data:84 A9 61 00 02 30 77 0D
//Receive	Data:84 A9 61 00 04 30 76 7f 5d d5
Receive	Data:84 A9 61 00 04 30 76 00 00 00
Receive	Data:84 A9 61 00 04 30 50 12 D6 87
Receive	Data:84 A9 61 00 04 30 51 12 D6 87
Receive	Data:84 A9 61 00 05 30 7d 01 23 45 67
Receive	Data:84 A9 61 00 05 30 7e 01 23 45 67
Receive	Data:84 A9 61 00 02 30 27 00
pause 1500
Command ID:	DMR_CALL_STOP
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Data:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Pause 2000


Command ID:	CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 01
Receive	Data:84 A9 61 00 02 03 19 00
Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00

Command ID: WORK_MODE_BER
Send command: 84 A9 61 00 04 00 18 03 00 01
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: WORK_MODE_BER
Send command: 84 A9 61 00 04 00 18 03 00 02
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: WORK_MODE_BER
Send command: 84 A9 61 00 04 00 18 03 00 03
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: ALOOP_CODEC_LOOP
Send command: 84 A9 61 00 04 00 18 03 01 00
Receive Data: 84 A9 61 00 02 00 18 00
