//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//

 .Set x = FF BF 
 .Set y = 17 04
 .set z = 17 06

// This command file assume layer12 build is loaded 
// It also assume activation code 7 is used

Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Command:84 A9 61 00 02 00 18 00

Command ID:	PROTOCOL_OPTION  
Send	Command: 84 A9 61 00 02 00 55 80
Receive	Data:84 A9 61 00 02 00 55 00
Command ID:	  VOCODER_CMODE1
Send Command: 84 A9 61 00 01 00 02 AA
Receive Data: 84 A9 61 00 02 00 {z}

Command ID:	  VOCODER_CMODE2
Send Command: 84 A9 61 00 03 00 02 {x}
Receive Data: 84 A9 61 00 02 00 17 04
//Receive Data: 84 A9 61 00 02 00 05 00
Command ID:  	VOCODER_CMODE3
Send Command: 84 A9 61 00 01 20 02 
Receive Data: 84 A9 61 00 02 20 17 06


Command ID: 	VOCODER_TONE1
Send Command: 84 A9 61 00 02 00 08 01 80 F3 
Receive Data: 84 A9 61 00 02 00 {z}
Command ID:	  VOCODER_TONE2
Send Command: 84 A9 61 00 06 00 08 01 80 F3 {x}
Receive Data: 84 A9 61 00 02 00 17 04
Command ID: 	VOCODER_TONE3
Send Command: 84 A9 61 00 01 20 08 
Receive Data: 84 A9 61 00 04 20 08 01 80 F3

Command ID:	  VOCODER_SEL1
Send Command: 84 A9 61 00 01 00 10 03
Receive Data: 84 A9 61 00 02 00 {z}
//Command ID:	  VOCODER_SEL2
//Send Command: 84 A9 61 00 04 00 10 00 {x}
//Receive Data: 84 A9 61 00 02 00 17 04
//Command ID:	  VOCODER_SEL3
//Send Command: 84 A9 61 00 01 20 10
//Receive Data: 84 A9 61 00 02 20 10 03
Command ID:   VOCODER_INI1
Send command: 84 A9 61 00 01 00 12 03
Receive Data: 84 A9 61 00 02 00 {z}
Command ID:   VOCODER_INI2
Send command: 84 A9 61 00 03 00 12 {x}
Receive Data: 84 A9 61 00 02 00 17 04
Command ID:   VOCODER_INI3
Send command: 84 A9 61 00 01 20 12
Receive Data: 84 A9 61 00 02 20 17 06




//Command ID: CHIP_RESET
//Send command: 84 A9 61 00 01 00 14
//Receive Data: 84 A9 61 00 02 33 17 01
//PAUSE 1000
//Command ID: LOW_POWER
//Send command: 84 A9 61 00 02 00 15 00
//Receive Data: 84 A9 61 00 02 00 15 00
//PAUSE 300


Command ID:   WORK_MODE1
Send command: 84 A9 61 00 02 00 18 00 00 00
Receive Data: 84 A9 61 00 02 00 {z}
Command ID:   WORK_MODE2
Send command: 84 A9 61 00 06 00 18 00 00 00 {x}
Receive Data: 84 A9 61 00 02 00 17 04
Command ID:   WORK_MODE3
Send command: 84 A9 61 00 01 20 18
Receive Data: 84 A9 61 00 04 20 18 00 00 00

Command ID:   CARRIER_READY1
Send command: 84 A9 61 00 01 00 19 01
Receive Data: 84 A9 61 00 02 00 {z}
Command ID:   CARRIER_READY2
Send command: 84 A9 61 00 04 00 19 01 {x}
Receive Data: 84 A9 61 00 02 00 17 04
Command ID:   CARRIER_READY3
Send command: 84 A9 61 00 01 20 19
Receive Data: 84 A9 61 00 02 20 17 06

Command ID:   PROCESS_MODE1
Send command: 84 A9 61 00 01 00 1A 01
Receive Data: 84 A9 61 00 02 00 {z}
Command ID:   PROCESS_MODE2
Send command: 84 A9 61 00 04 00 1A 01 {x}
Receive Data: 84 A9 61 00 02 00 17 04
Command ID:   PROCESS_MODE3
Send command: 84 A9 61 00 01 20 1A
Receive Data: 84 A9 61 00 02 20 17 06
Command ID:   PROCESS_MODE4
Send command: 84 A9 61 00 02 00 1A 03
Receive Data: 84 A9 61 00 02 00 1A 00

PAUSE 500
Command ID:   DEMOD_GAIN1
Send command: 84 A9 61 00 02 00 1C 00 00
Receive Data: 84 A9 61 00 02 00 {z}
Command ID:   DEMOD_GAIN2
Send command: 84 A9 61 00 05 00 1C 00 00 {x}
Receive Data: 84 A9 61 00 02 00 17 04
Command ID:   DEMOD_GAIN3
Send command: 84 A9 61 00 01 20 1C 
Receive Data: 84 A9 61 00 03 20 1C 08 00

Command ID:   REPORT_FIELD1
Send command: 84 A9 61 00 01 00 1D 70
Receive Data: 84 A9 61 00 02 00 {z}
Command ID:   REPORT_FIELD2
Send command: 84 A9 61 00 04 00 1D 70 {x}
Receive Data: 84 A9 61 00 02 00 17 04
Command ID:   REPORT_FIELD3
Send command: 84 A9 61 00 01 20 1D 
Receive Data: 84 A9 61 00 02 20 17 06

Command ID:	  READ_BER_REPORT1
Send Command: 84 A9 61 00 01 00 1E 00
Receive Data: 84 A9 61 00 02 00 17 06
Command ID:  	READ_BER_REPORT2
Send Command: 84 A9 61 00 02 20 1E 00
Receive Data: 84 A9 61 00 0C 20 1E 00 00 00 00 00 00 00 00 00 00 00

Command ID:	  LOCAL_TONE1
Send Command: 84 A9 61 00 11 00 1F 01 03 E8 07 D0 04 B0 05 DC 20 20 20 20 03 E8 03 E8
Receive Data: 84 A9 61 00 02 00 {z}
Command ID:	  LOCAL_TONE2
Send Command: 84 A9 61 00 14 00 1F 01 03 E8 07 D0 04 B0 05 DC 20 20 20 20 03 E8 03 E8 {x}
Receive Data: 84 A9 61 00 02 00 17 04
Command ID:	  LOCAL_TONE3
Send Command: 84 A9 61 00 01 20 1F
Receive Data: 84 A9 61 00 02 20 17 06

Command ID:  	ADDRESSING_MODE
Send Command: 84 A9 61 00 02 03 28 01
Receive Data: 84 A9 61 00 02 03 28 00
Command ID:   DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 12 34 56
Receive Data: 84 A9 61 00 02 03 50 00
Command ID:   DPMR_OWN_ID
Send command: 84 A9 61 00 04 03 51 11 22 33
Receive Data: 84 A9 61 00 02 03 51 00
Command ID:   READ_DPMR_CALLED_OWN_ID
Send command: 84 A9 61 00 02 23 50 51
Receive Data: 84 A9 61 00 04 23 50 12 34 56
Receive Data: 84 A9 61 00 04 23 51 11 22 33
Command ID:   RFAR_DPMR_CALLED_OWN_ID
Send command: 84 A9 61 00 02 33 50 51
Receive Data: 84 A9 61 00 04 33 50 00 00 00
Receive Data: 84 A9 61 00 04 33 51 00 00 00
Command ID:   DPMR_CALLED_ID_BCD
Send command: 84 A9 61 00 05 03 52 12 34 56 70
Receive Data: 84 A9 61 00 02 03 52 00
Command ID:   DPMR_OWN_ID_BCD
Send command: 84 A9 61 00 05 03 53 11 22 33 44
Receive Data: 84 A9 61 00 02 03 53 00
Command ID:   READ_DPMR_CALLED_OWN_BCD
Send command: 84 A9 61 00 02 23 52 53
Receive Data: 84 A9 61 00 05 23 52 12 34 56 70
Receive Data: 84 A9 61 00 05 23 53 11 22 33 40
Command ID:   RFAR_DPMR_CALLED_OWN_BCD
Send command: 84 A9 61 00 02 33 52 53
Receive Data: 84 A9 61 00 05 33 52 00 00 00 00
Receive Data: 84 A9 61 00 05 33 53 00 00 00 00

Command ID:  	CALL_START1
Send Command: 84 A9 61 00 01 00 20 12
Receive Data: 84 A9 61 00 02 00 {z}
Command ID:	  CALL_START2
Send Command: 84 A9 61 00 04 00 20 02 {x}
Receive Data: 84 A9 61 00 02 00 17 04
Command ID:	  CALL_START3
Send Command: 84 A9 61 00 01 20 20
Receive Data: 84 A9 61 00 02 20 17 06


Command ID:	  CALL_STOP1
Send Command: 84 A9 61 00 01 00 21 00
Receive Data: 84 A9 61 00 02 00 21 00
Command ID:	  CALL_STOP2
Send Command: 84 A9 61 00 03 00 21 {x} 
Receive Data: 84 A9 61 00 02 00 17 04
Command ID:	  CALL_STOP3
Send Command: 84 A9 61 00 01 20 21 
Receive Data: 84 A9 61 00 02 20 17 06


Command ID:	  CONNECT1
Send Command: 84 A9 61 00 01 00 22 13
Receive Data: 84 A9 61 00 02 00 {z}
Command ID:	  CONNECT2
Send Command: 84 A9 61 00 04 00 22 13 {x}
Receive Data: 84 A9 61 00 02 00 17 04
Command ID:	  CONNECT3
Send Command: 84 A9 61 00 01 20 22
Receive Data: 84 A9 61 00 02 20 17 06

                                         
Command ID:	  DISCONNECT1                  
Send Command: 84 A9 61 00 01 00 23 12    
Receive Data: 84 A9 61 00 02 00 {z}      
Command ID:	  DISCONNECT2                  
Send Command: 84 A9 61 00 04 00 23 12 {x}
Receive Data: 84 A9 61 00 02 00 17 04    
Command ID:	  DISCONNECT3                  
Send Command: 84 A9 61 00 01 20 23       
Receive Data: 84 A9 61 00 02 20 17 06                                       
                                                                                                       
                                                                                                                   
Command ID:	  DPMR_ACK1                                                                                              
Send Command: 84 A9 61 00 01 00 24 12                                                                              
Receive Data: 84 A9 61 00 02 00 {z}                                                                                
Command ID:	  DPMR_ACK2                                                                                              
Send Command: 84 A9 61 00 04 00 24 12 {x}                                                                          
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:	  DPMR_ACK3                                                                                              
Send Command: 84 A9 61 00 01 20 24                                                                                 
Receive Data: 84 A9 61 00 02 20 17 06                                                                              
                                                                                                                   
                                                                                                                   
Command ID:	  SYS_INFO1                                                                                              
Send Command: 84 A9 61 00 01 00 25 12                                                                              
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:	  SYS_INFO2                                                                                              
Send Command: 84 A9 61 00 04 00 25 12 {x}                                                                          
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:	  SYS_INFO3                                                                                              
Send Command: 84 A9 61 00 01 20 25                                                                                 
Receive Data: 84 A9 61 00 02 20 17 06                                                                              
                                                                                                                   
                                                                                                                   
Command ID:	  CALL_MATCH1                                                                                            
Send Command: 84 A9 61 00 01 20 27                                                                                 
Receive Data: 84 A9 61 00 02 20 17 04                                                                              
                                                                                                                   
Command ID:	  ADDRESSING_MODE1                                                                                     
Send Command: 84 A9 61 00 01 00 28 01                                                                              
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:	  ADDRESSING_MODE2                                                                                     
Send Command: 84 A9 61 00 04 00 28 01 {x}                                                                          
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:	  ADDRESSING_MODE3                                                                                     
Send Command: 84 A9 61 00 01 20 28                                                                                 
Receive Data: 84 A9 61 00 02 20 17 06                                                                              
                                                                                                                   
Command ID:	  GROUP_ID1                                                                                          
Send Command: 84 A9 61 00 04 00 29 12 34 56 92 00                                                                
Receive Data: 84 A9 61 00 02 00 17 06                                                                            
Command ID:	  GROUP_ID2                                                                                          
Send Command: 84 A9 61 00 07 00 29 12 34 56 92 {x}                                                               
Receive Data: 84 A9 61 00 02 00 17 04                                                                            
Command ID:	  GROUP_ID3                                                                                          
Send Command: 84 A9 61 00 02 20 29 00    //group number is 0?                                                                          
Receive Data: 84 A9 61 00 02 20 17 06                                                                 
PAUSE 500
                                                                                                                   
//Command ID:   SCRAMBLER_SEED1                                                                                    
//Send Command: 84 A9 61 00 19 00 2A 03 12 34 45 78 9A BC DE F0 00 11 22 33 44 55 66 77 88 99 AA BB CC DD EE FF    
//Receive Data: 84 A9 61 00 02 00 2A 05                                                                            
//Command ID:   SCRAMBLER_SEED2                                                                                    
//Send Command: 84 A9 61 00 1C 00 2A 03 12 34 45 78 9A BC DE F0 00 11 22 33 44 55 66 77 88 99 AA BB CC DD EE FF {x}
//Receive Data: 84 A9 61 00 02 00 17 04                                                                            
//Command ID:   SCRAMBLER_SEED3                                                                                    
//Send Command: 84 A9 61 00 01 20 2A                                                                               
//Receive Data: 84 A9 61 00 02 20 17 06                                                                            
                                                                                                                   
Command ID:	  MODEL_SEL1                                                                                           
Send Command: 84 A9 61 00 01 00 2B 01                                                                              
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:	  MODEL_SEL2                                                                                           
Send Command: 84 A9 61 00 04 00 2B 00 {x}                                                                          
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:	  MODEL_SEL3                                                                                           
Send Command: 84 A9 61 00 01 20 2B                                                                                 
Receive Data: 84 A9 61 00 02 20 2B 00                                                                              
                                                                                                                   
Command ID:	  MOD_GAIN1                                                                                            
Send Command: 84 A9 61 00 02 00 2C 00 01                                                                           
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:	  MOD_GAIN2                                                                                            
Send Command: 84 A9 61 00 05 00 2C 00 01 {x}                                                                       
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:	  MOD_GAIN3                                                                                            
Send Command: 84 A9 61 00 01 20 2C                                                                                 
Receive Data: 84 A9 61 00 02 20 17 06                                                                              
                                                                                                                   
//Command ID:	  CODEC_SELECT1                                                                                      
//Send Command: 84 A9 61 00 01 00 2D 02                                                                            
//Receive Data: 84 A9 61 00 02 00 {y}                                                                            
//Command ID:	  CODEC_SELECT2                                                                                      
//Send Command: 84 A9 61 00 04 00 2D 02 {x}                                                                        
//Receive Data: 84 A9 61 00 02 00 17 04                                                                            
//Command ID:	  CODEC_SELECT3                                                                                      
//Send Command: 84 A9 61 00 01 20 2D                                                                               
//Receive Data: 84 A9 61 00 02 20 17 06                                                                            
                                                                                                                   
Command ID:	  I2C_ADDRESS1                                                                                         
Send Command: 84 A9 61 00 01 00 2E FF                                                                              
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:	  I2C_ADDRESS2                                                                                         
Send Command: 84 A9 61 00 04 00 2E FF {x}                                                                          
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:	  I2C_ADDRESS3                                                                                         
Send Command: 84 A9 61 00 01 20 2E                                                                                 
Receive Data: 84 A9 61 00 02 20 17 06                                                                              
                                                                                                                   
Command ID:	  SYNC_COUNT1                                                                                          
Send Command: 84 A9 61 00 01 00 2F 01                                                                              
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:	  SYNC_COUNT2                                                                                          
Send Command: 84 A9 61 00 04 00 2F 01 {x}                                                                          
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:	  SYNC_COUNT3                                                                                          
Send Command: 84 A9 61 00 01 20 2F                                                                                 
Receive Data: 84 A9 61 00 02 20 17 06                                                                              
                                                                                                                   
Command ID:    Q_PRO_VER2                                                                                          
Send Command: 84 A9 61 00 01 00 30 FF FF 00                                                                        
Receive	Data: 84 A9 61 00 02 00 17 06                                                                              
                                                                                                                   
Command ID:   Q_HW_VER1                                                                                            
Send command: 84 A9 61 00 01 20 31                                                                                 
Receive Data: 84 A9 61 00 0A 20 31 08 56 30 2E 30 31 2E 30 32                                                      
Command ID:   Q_HW_VER2                                                                                            
Send Command: 84 A9 61 00 01 00 31 FF FF 00                                                                        
Receive	Data: 84 A9 61 00 02 00 17 06                                                                              
                                                                                                                   
                                                                                                                   
Command ID:   Q_SW_VER2                                                                                            
Send Command: 84 A9 61 00 01 00 32 FF FF 00                                                                        
Receive	Data: 84 A9 61 00 02 00 17 06                                                                              
                                                                                                                   
                                                                                                                   
Command ID:   Q_CID_SN2                                                                                            
Send Command: 84 A9 61 00 01 00 33 FF FF 00                                                                        
Receive	Data: 84 A9 61 00 02 00 17 06                                                                              
                                                                                                                   
Command ID:	  Q_FID2                                                                                               
Send Command: 84 A9 61 00 01 00 34 FF FF 00                                                                        
Receive	Data: 84 A9 61 00 02 00 17 06                                                                              
                                                                                                                   
Command ID:	  Q_USE_NUMBER2                                                                                        
Send Command: 84 A9 61 00 02 00 34 FF FF 00                                                                        
Receive	Data: 84 A9 61 00 02 00 17 06                                                                              
                                                                                                                   
Command ID:	  DC_OFFSET1                                                                                           
Send Command: 84 A9 61 00 0C 00 39 80 00 80 00 80 00 80 00 00 00 00 00                                             
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:	  DC_OFFSET2                                                                                           
Send Command: 84 A9 61 00 0f 00 39 80 00 80 00 80 00 80 00 00 00 00 00 {x}                                         
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:	  DC_OFFSET3                                                                                           
Send Command: 84 A9 61 00 01 20 39                                                                                 
Receive Data: 84 A9 61 00 02 20 17 06                                                                              
                                                                                                                   
Command ID:	  DCCOMP_FILTER1                                                                                       
Send Command: 84 A9 61 00 01 00 3B 00 00 00 00 00                                                                  
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:	  DCCOMP_FILTER2                                                                                       
Send Command: 84 A9 61 00 07 00 3B 00 00 00 00 {x}                                                                 
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:	  DCCOMP_FILTER                                                                                        
Send Command: 84 A9 61 00 01 20 3B 00                                                                              
Receive	Data: 84 A9 61 00 02 20 17 06                                                                              
                                                                                                                   
Command ID: 	ANALOG_CONFIG1                                                                                       
Send Command: 84 A9 61 00 0A 00 3C 02 08 00 40 00 02 3D 10 00 08 00                                                
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:  	ANALOG_CONFIG2                                                                                       
Send Command: 84 A9 61 00 0D 00 3C 02 08 00 40 00 02 3D 10 00 08 00 {x}                                            
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:	  ANALOG_CONFIG3                                                                                       
Send Command: 84 A9 61 00 01 20 3C                                                                                 
Receive Data: 84 A9 61 00 02 20 17 06                                                                              
 
Command ID: 	VOX_ENERGY1
Send Command: 84 A9 61 00 02 00 3d 00 00
Receive Data: 84 A9 61 00 02 00 {z} 
Command ID: 	VOX_ENERGY2
Send Command: 84 A9 61 00 05 00 3d 00 00 {x}
Receive	Data: 84 A9 61 00 02 00 17 04
//Command ID: 	VOX_ENERGY3
//Send Command: 84 A9 61 00 01 20 3d
//Receive Data: 84 A9 61 00 03 20 3D 00 F0
                                                                                                                                                                                                                                                                                                                                                         
Command ID:	  NUM_PREAMBLE1                                                                                        
Send Command: 84 A9 61 00 02 00 46 0A 0A 00                                                                        
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:	  NUM_PREAMBLE2                                                                                        
Send command: 84 A9 61 00 05 00 46 0A 0A {x}                                                                       
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:	  NUM_PREAMBLE3                                                                                        
Send command: 84 A9 61 00 01 20 46                                                                                 
Receive Data: 84 A9 61 00 02 20 17 06                                                                              
                                                                                                                      
Command ID:   DPMR_END_UE1                                                                                         
Send command: 84 A9 61 00 03 03 4B 33 44 FF                                                                        
Receive Data: 84 A9 61 00 02 03 {z}                                                                              
Command ID:   DPMR_END_UE2                                                                                         
Send command: 84 A9 61 00 06 03 4B 33 44 FF {x}                                                                    
Receive Data: 84 A9 61 00 02 03 17 04                                                                              
Command ID:   DPMR_END_UE3                                                                                         
Send command: 84 A9 61 00 01 20 4B                                                                                 
Receive Data: 84 A9 61 00 04 20 4B 33 44 FF                                                                       
                                                                                                                   
Command ID:   DPMR_FS11                                                                                            
Send command: 84 A9 61 00 06 03 4C 57 77 5F 75 D5 FF                                                               
Receive Data: 84 A9 61 00 02 03 {z}                                                                              
Command ID:   DPMR_FS12                                                                                            
Send command: 84 A9 61 00 09 03 4C 57 77 5F 75 D5 FF {x}                                                           
Receive Data: 84 A9 61 00 02 03 17 04                                                                              
Command ID:   DPMR_FS13                                                                                            
Send command: 84 A9 61 00 01 23 4C                                                                                 
Receive Data: 84 A9 61 00 07 23 4C 57 77 5F 75 D5 FF                                                               
                                                                                                                   
Command ID:   DPMR_FS21                                                                                            
Send command: 84 A9 61 00 03 03 4D 5F 7D F7                                                                        
Receive Data: 84 A9 61 00 02 03 {z}                                                                              
Command ID:   DPMR_FS22                                                                                            
Send command: 84 A9 61 00 06 03 4D 5F 7D F7 {z}                                                                    
Receive Data: 84 A9 61 00 02 03 17 06                                                                              
Command ID:   DPMR_FS23                                                                                            
Send command: 84 A9 61 00 01 23 4D                                                                                 
ReceiveData : 84 A9 61 00 04 23 4D 5F 7D F7                                                                       
                                                                                                                   
Command ID:   DPMR_FS31                                                                                            
Send command: 84 A9 61 00 03 03 4E 7D F5 DF                                                                        
Receive Data: 84 A9 61 00 02 03 {z}                                                                              
Command ID:   DPMR_FS32                                                                                            
Send command: 84 A9 61 00 06 03 4E 7D F5 DF {x}                                                                    
Receive Data: 84 A9 61 00 02 03 {y}                                                                             
Command ID:   DPMR_FS33                                                                                            
Send command: 84 A9 61 00 01 23 4E                                                                                 
ReceiveData : 84 A9 61 00 04 23 4E 7D F5 DF                                                                       
                                                                                                                   
Command ID:   DPMR_FS41                                                                                            
Send command: 84 A9 61 00 06 03 4F FD 55 F5 DF DD 7F 00                                                            
Receive Data: 84 A9 61 00 02 03 {z}                                                                              
Command ID:   DPMR_FS42                                                                                            
Send command: 84 A9 61 00 09 03 4F FD 55 F5 DF DD 7F {x}                                                           
Receive Data: 84 A9 61 00 02 03 {y}                                                                              
Command ID:   DPMR_FS43                                                                                            
Send command: 84 A9 61 00 01 23 4F                                                                                 
ReceiveData : 84 A9 61 00 07 23 4F FD 55 F5 DF DD 7F                                                              
                                                                                                                   
Command ID:   DPMR_CALLED_ID1                                                                                      
Send command: 84 A9 61 00 03 03 50 12 34 56                                                                        
Receive Data: 84 A9 61 00 02 03 {z}                                                                              
Command ID:   DPMR_CALLED_ID2                                                                                      
Send command: 84 A9 61 00 05 03 50 12 34 56 {x}                                                                    
Receive Data: 84 A9 61 00 02 03 {y}                                                                              
Command ID:   DPMR_CALLED_ID3                                                                                      
Send command: 84 A9 61 00 01 23 50                                                                                 
Receive Data: 84 A9 61 00 04 23 50 12 34 56                                                                        
                                                                                                                   
Command ID:   DPMR_OWN_ID1                                                                                         
Send command: 84 A9 61 00 03 03 51 11 22 33                                                                        
Receive Data: 84 A9 61 00 02 03 {z}                                                                              
Command ID:   DPMR_OWN_ID2                                                                                         
Send command: 84 A9 61 00 06 03 51 11 22 33 {x}                                                                    
Receive Data: 84 A9 61 00 02 03 17 04                                                                              
Command ID:   DPMR_OWN_ID3                                                                                         
Send command: 84 A9 61 00 01 23 51                                                                                 
Receive Data: 84 A9 61 00 04 23 51 11 22 33                                                                        
                                                                                                                   
Command ID:   DPMR_CALLED_ID_BCD1                                                                                  
Send command: 84 A9 61 00 04 03 52 12 34 56 70                                                                     
Receive Data: 84 A9 61 00 02 03 {z}                                                                              
Command ID:   DPMR_CALLED_ID_BCD2                                                                                  
Send command: 84 A9 61 00 07 03 52 12 34 56 70 {x}                                                                 
Receive Data: 84 A9 61 00 02 03 17 04                                                                              
Command ID:   DPMR_CALLED_ID_BCD3                                                                                  
Send command: 84 A9 61 00 01 23 52                                                                                 
Receive Data: 84 A9 61 00 05 23 52 12 34 56 70                                                                     
                                                                                                                   
Command ID:   DPMR_OWN_ID_BCD1                                                                                     
Send command: 84 A9 61 00 04 03 53 11 22 33 44                                                                     
Receive Data: 84 A9 61 00 02 03 {z}                                                                              
Command ID:   DPMR_OWN_ID_BCD2                                                                                     
Send command: 84 A9 61 00 07 03 53 11 22 33 44 {x}                                                                 
Receive Data: 84 A9 61 00 02 03 17 04                                                                              
Command ID:   DPMR_OWN_ID_BCD3                                                                                     
Send command: 84 A9 61 00 01 23 53                                                                                 
Receive Data: 84 A9 61 00 05 23 53 11 22 33 40                                                                     
                                                                                                                   
Command ID:   DPMR_M_F1                                                                                            
Send command: 84 A9 61 00 01 03 54 02                                                                              
Receive Data: 84 A9 61 00 02 03 {z}                                                                              
Command ID:   DPMR_M_F2                                                                                            
Send command: 84 A9 61 00 04 03 54 02 {x}                                                                          
Receive Data: 84 A9 61 00 02 03 17 04                                                                              
Command ID:   DPMR_M_F3                                                                                            
Send command: 84 A9 61 00 01 23 54                                                                                 
Receive Data: 84 A9 61 00 02 23 54 02                                                                              
                                                                                                                   
Command ID:   DPMR_SLD1                                                                                            
Send command: 84 A9 61 00 03 03 56 11 22 FF                                                                        
Receive Data: 84 A9 61 00 02 03 {z}                                                                              
Command ID:   DPMR_SLD2                                                                                            
Send command: 84 A9 61 00 06 03 56 11 22 FF {x}                                                                    
Receive Data: 84 A9 61 00 02 03 17 04                                                                              
Command ID:   DPMR_SLD3                                                                                            
Send command: 84 A9 61 00 01 23 56                                                                                 
ReceiveData:  84 A9 61 00 04 23 56 00 80 40                                                                    
                                                                                                                   
Command ID:   DPMR_CC1
Send command: 84 A9 61 00 03 03 5C 77 F5 D5
Receive Data: 84 A9 61 00 02 03 {z}
Command ID:   DPMR_CC2
Send command: 84 A9 61 00 06 03 5C 77 F5 D5 {x}
Receive Data: 84 A9 61 00 02 03 17 04
Command ID:   DPMR_CC3
Send command: 84 A9 61 00 01 23 5C
Receive Data: 84 A9 61 00 04 23 5C 77 F5 D5


Command ID:   DPMR_SEND_SF1
Send command: 84 A9 61 00 01 03 5F 
Receive Data: 84 A9 61 00 02 03 5F 00
Command ID:   DPMR_SEND_SF2
Send command: 84 A9 61 00 03 03 5F {x}
Receive Data: 84 A9 61 00 02 03 17 04
Command ID:   DPMR_SEND_SF3
Send command: 84 A9 61 00 01 23 5F 
Receive	Data: 84 A9 61 00 02 23 17 06

Command ID:   DPMR_SEND_HEADER1
Send command: 84 A9 61 00 01 03 60 
Receive Data: 84 A9 61 00 02 03 60 00
Command ID:   DPMR_SEND_HEADER2
Send command: 84 A9 61 00 03 03 60 {x}
Receive Data: 84 A9 61 00 02 03 17 04
Command ID:   DPMR_SEND_HEADER3
Send command: 84 A9 61 00 01 23 60 
Receive Data: 84 A9 61 00 02 23 17 06
  
Command ID:   DPMR_SEND_END1  
Send command: 84 A9 61 00 01 03 61 
Receive Data: 84 A9 61 00 02 03 61 00 
Command ID:   DPMR_SEND_END2  
Send command: 84 A9 61 00 03 03 61 {x}
Receive Data: 84 A9 61 00 02 03 17 04
Command ID:   DPMR_SEND_END3  
Send command: 84 A9 61 00 01 23 61 
Receive Data: 84 A9 61 00 02 23 17 06   



Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 09 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 0A 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:  	 Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 0B 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 0C 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 0D 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 0E 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 0F 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 36 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 37 00
Receive	Data:  84 A9 61 00 02 00 17 06

Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 6B 00
Receive	Data:  84 A9 61 00 02 00 17 06
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 6C 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 6D 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 6E 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 6F 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 76 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 77 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 78 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 79 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 7A 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 7B 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 7C 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 7D 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 7E 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 7F 00
Receive	Data:  84 A9 61 00 02 00 17 04


Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 84 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 85 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 86 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 87 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 88 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 89 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 8A 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 8B 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 8C 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 8D 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 8E 00
Receive	Data:  84 A9 61 00 02 00 17 04
Command ID:	   Unsupported Filed ID1
Send	Command: 84 A9 61 00 02 00 8F 00
Receive	Data:  84 A9 61 00 02 00 17 04



                                                                                                            
//Command ID:	VOCODER_CMODE_PARITY                                                                                 
//Send Command: 84 A9 61 00 04 00 02 0C 2F 25                                                                      
//Receive Data: 84 A9 61 00 04 00 02 00 2F 29                                                                      
                                                                                                                   
//Command ID:	 CHAN_NUM_SAMPLE_PARITY                                                                              
//Send Command: 84 A9 61 00 04 00 03 00 2F 28                                                                      
//Receive Data: 84 A9 61 00 04 00 03 00 2F 28                                                                      
                                                                                                                   
//Command ID:   VOCODER_INI4                                                                                       
//Send	Command: 84 A9 61 00 04 00 12 03 2F 3A                                                                     
//Receive Data: 84 A9 61 00 04 00 12 00 2F 39                                                                      
                                                                                                                   
//Command ID:	VOCODER_TONE4                                                                                        
//Send Command: 84 A9 61 00 06 00 08 01 80 F3 2F 53                                                                
//Receive Data: 84 A9 61 00 04 00 08 00 2F 23                                                                      