//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Button PLLBYPASS1 // SET HIGH 
//Button PLLBYPASS0 // SET LOW 
//Button PLLSEL1  // SET HIGH 
//Button PLLSEL0  // SET LOW 
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
//Codec selection
Command ID: CODEC_SEL
Send Command: 84 A9 61 00 02 03 2D 33
//Send Command: 84 A9 61 00 02 03 2D 03
Receive Data: 84 A9 61 00 02 03 2D 00
Pause 1000
//Vocoder selection
//Command ID: VOCODER_SEL
//Send Command: 84 A9 61 00 02 00 10 00
//Receive Data:84 A9 61 00 02 00 10 00
//Receive Data:84 A9 61 00 03 00 39 2f 15
//Pause 2000
Command ID:	CALL_OPTION
//Send	Command: 84 A9 61 00 06 05 47 01 80 00 00 00
Send	Command: 84 A9 61 00 06 05 47 70 80 00 00 00
Receive	Command:84 A9 61 00 02 05 47 00
Pause 2000
//Freq set: (F *2^20)/36.864
Command ID:	spi3700_freq  446M Mhz
//Send	Command: 84 A9 61 00 03 00 6D 01 c1 00
Send	Command: 84 A9 61 00 03 00 6D 01 b4 00
 Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	spi3700_freq
//Send	Command: 84 A9 61 00 03 00 6D 02 93 00
Send	Command: 84 A9 61 00 03 00 6D 02 1f 00
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	spi3700_freq
//Send	Command: 84 A9 61 00 03 00 6D 03 8e 00
Send	Command: 84 A9 61 00 03 00 6D 03 1c 00
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	spi3700_freq
//Send	Command: 84 A9 61 00 03 00 6D 04 C1 00
Send	Command: 84 A9 61 00 03 00 6D 04 b4 00
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	spi3700_freq
//Send	Command: 84 A9 61 00 03 00 6D 05 93 00
Send	Command: 84 A9 61 00 03 00 6D 05 1f 00
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	spi3700_freq
//Send	Command: 84 A9 61 00 03 00 6D 06 8E 00
Send	Command: 84 A9 61 00 03 00 6D 06 1c 00
Receive	Data:84 A9 61 00 02 00 6D 00
//Set SR for local side
//Command ID: NXDN_SR
//Send Command: 84 A9 61 00 02 05 77 01
//Receive Data:84 A9 61 00 02 05 77 00
//PROCESS mode: layer 2 mode
Command ID: PROCESS_MODE
Send Command: 84 A9 61 00 02 00 1A 02
Receive Data:84 A9 61 00 02 00 1A 00

//
//Command ID: DMR_CALL_OPTION
Command ID:	WRITE_SQLEVEL
Send	Command: 84 A9 61 00 0D 00 6C 00 00 00 30 10 00 04 00 04 00 01 00 00
Receive	Data:84 A9 61 00 02 00 6C 00

