//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Button PLLBYPASS1 // SET HIGH 
//Button PLLBYPASS0 // SET LOW 
//Button PLLSEL1  // SET HIGH 
//Button PLLSEL0  // SET LOW 
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//


Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 06 00 6D 01 2E 02 04 08
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 05 00 6D 01 76 01 26
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 05 00 6D 01 7A 01 1C
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 05 00 6D 01 4D 01 09
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 06 00 6D 01 6A 02 00 01
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 06 00 6D 01 39 02 00 1B
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 06 00 6D 01 3A 02 C9 41
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 05 00 6D 01 40 01 03
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 05 00 6D 01 41 01 00
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 05 00 6D 01 42 01 0C
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 06 00 6D 01 2E 02 04 A9
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	Q_PRO_VER
Send	Command: 84 A9 61 00 02 05 2B 51
Receive	Data:84 A9 61 00 02 05 2B 00
