//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Button PLLBYPASS1 // SET HIGH 
//Button PLLBYPASS0 // SET LOW 
//Button PLLSEL1  // SET HIGH 
//Button PLLSEL0  // SET LOW 
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
Command ID: WORK_MODE_Tx
Send command: 84 A9 61 00 04 00 18 02 00 00
Receive Data: 84 A9 61 00 02 00 18 00
// Set single frame for voice call
Command ID: DIGC_DATA_FRAME
Send command: 84 a9 61 00 11 00 77 c1 43 a0 00 0b 40 01 00 20 00 04 00 01 00 00 00 00 
Receive Data: 84 a9 61 00 01 20 43
/*Command ID: DIGC_DATA_FRAME
Send command: 84 a9 61 00 11 02 77 00 43 a0 00 0b 40 01 00 80 00 01 00 02 00 00 00 00
Receive Data: 84 a9 61 00 01 20 43
Command ID: DIGC_DATA_FRAME
Send command: 84 a9 61 00 11 02 77 00 43 a0 00 0b 40 01 00 80 00 01 00 02 00 00 00 00
Receive Data: 84 a9 61 00 01 20 43
Command ID: DIGC_DATA_FRAME
Send command: 84 a9 61 00 11 02 77 00 43 a0 00 0b 40 01 00 80 00 01 00 02 00 00 00 00
Receive Data: 84 a9 61 00 01 20 43
Command ID: DIGC_DATA_FRAME
Send command: 84 a9 61 00 11 02 77 00 43 a0 00 0b 40 01 00 80 00 03 00 02 00 00 00 00
Receive Data: 84 a9 61 00 01 20 43*/
//Send superframe voice call
//Command ID: DIGC_DATA_FRAME
//Send command: 84 a9 61 00 10 02 77 c1 43 c0 00 0a 56 01 00 80 00 01 00 02 00 00
//Receive Data: 84 a9 61 00 01 20 43
Command ID: DIGC_DATA_FRAME
Send command: 84 a9 61 00 02 00 77 c1 
Receive Data: 84 a9 61 00 02 00 77 00
Command ID: DIGC_DATA_FRAME
Send command: 84 a9 61 00 0e 00 43 c0 00 0a 56 01 00 20 00 04 00 01 00 00
Receive Data: 84 a9 61 00 01 20 43
