//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//


.Set READY_VAR = 02
Command ID: PROCESS_MODE
Send command: 84 A9 61 00 02 00 1A 02
Receive Data: 84 A9 61 00 02 00 1A 00
Command ID:	PROTOCOL_OPTION  
Send	Command: 84 A9 61 00 02 00 55 80
Receive	Data:84 A9 61 00 02 00 55 00
Command ID: REPORT_FIELD
Send command: 84 A9 61 00 02 00 1D 70
Receive Data: 84 A9 61 00 02 00 1D 00
Command ID:	ADDRESSING_MODE
Send	Command: 84 A9 61 00 02 03 28 01
Receive	Command:84 A9 61 00 02 03 28 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 12 34 56
Receive Data: 84 A9 61 00 02 03 50 00
/*Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 11 22 33
Receive Data: 84 A9 61 00 02 03 50 00*/
Command ID: DPMR_M_F
Send command: 84 A9 61 00 02 03 54 FF
Receive Data: 84 A9 61 00 02 03 54 00
Command ID: DPMR_HT_CI
Send command: 84 A9 61 00 03 03 57 01 FE
Receive Data: 84 A9 61 00 02 03 57 00
Command ID: DPMR_END_UE
Send command: 84 A9 61 00 04 03 4B 00 00 00
Receive Data: 84 A9 61 00 02 03 4B 00
Command ID: ALOOP_CODEC_LOOP
Send command: 84 A9 61 00 04 00 18 03 01 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: ALOOP_DECIMATOR_LOOP
Send command: 84 A9 61 00 04 00 18 03 02 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: ALOOP_VOCODER_LOOP
Send command: 84 A9 61 00 04 00 18 03 13 00
Receive Data: 84 A9 61 00 02 00 18 00
Pause 2000
Command ID: ALOOP_4FSK_LOOP
Send command: 84 A9 61 00 04 00 18 03 06 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500 
Command ID: DPMR_SEND_HEAD_SF
Send command: 84 A9 61 00 02 00 60 5F
Receive Data: 84 A9 61 00 02 00 5F 00
Receive Data: 84 A9 61 00 03 30 57 01 FE
Receive Data: 84 A9 61 00 02 30 54 FF
Receive Data: 84 A9 61 00 04 30 50 12 34 56
Pause 5000
Command ID: SEND_END_CLOST
Send command: 84 A9 61 00 03 00 61 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 20 17 0A
Pause 500
Command ID: SEND_SF_CREADY
Send command: 84 A9 61 00 03 00 5F 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
//Receive Data: 84 A9 61 00 03 30 57 01 FE
Receive Data: 84 A9 61 00 02 30 54 FF
Receive Data: 84 A9 61 00 04 30 50 12 34 56
Pause 3000
Command ID: DPMR_SEND_END
Send command: 84 A9 61 00 01 03 61
Receive Data: 84 A9 61 00 02 03 61 00
Receive Data: 84 A9 61 00 04 30 4B 00 00 00
Receive Data: 84 A9 61 00 02 20 17 0A
Pause 1000
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Command ID: WORK_MODE_BER
Send command: 84 A9 61 00 04 00 18 03 00 01
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: WORK_MODE_BER
Send command: 84 A9 61 00 04 00 18 03 00 02
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: WORK_MODE_BER
Send command: 84 A9 61 00 04 00 18 03 00 03
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: ALOOP_CODEC_LOOP
Send command: 84 A9 61 00 04 00 18 03 01 00
Receive Data: 84 A9 61 00 02 00 18 00
