//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
Command ID:	WM-0
Send	Command: 84 A9 61 00 02 40 00 00
Receive	Command:84 A9 61 00 02 40 17 00
pause 1000
Command ID:	WM-61
Send	Command: 84 A9 61 00 02 40 7B 00
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-52
Send	Command: 84 A9 61 00 02 40 69 40
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-53
Send	Command: 84 A9 61 00 02 40 6B 40
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-54
Send	Command: 84 A9 61 00 02 40 6D 40
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-55
Send	Command: 84 A9 61 00 02 40 6F 40
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-50
Send	Command: 84 A9 61 00 02 40 64 01
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-51
Send	Command: 84 A9 61 00 02 40 66 01
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-42
Send	Command: 84 A9 61 00 02 40 54 04
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-2
Send	Command: 84 A9 61 00 02 40 05 bF
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-3
Send	Command: 84 A9 61 00 02 40 06 6F
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-1
Send	Command: 84 A9 61 00 02 40 02 1D
Receive	Command:84 A9 61 00 02 40 17 00
Pause 100
Command ID:	WM-4
Send	Command: 84 A9 61 00 02 40 09 18
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-6
Send	Command: 84 A9 61 00 02 40 0C 4D
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-7
Send	Command: 84 A9 61 00 02 40 0F 04
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-10
Send	Command: 84 A9 61 00 02 40 14 00
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-14
Send	Command: 84 A9 61 00 02 40 1C 00
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM_44
Send	Command: 84 A9 61 00 02 40 58 33
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-45
Send	Command: 84 A9 61 00 02 40 5A 10
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-46
Send	Command: 84 A9 61 00 02 40 5D 10
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-47
Send	Command: 84 A9 61 00 02 40 5E 00
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-48
Send	Command: 84 A9 61 00 02 40 60 00
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-49
Send	Command: 84 A9 61 00 02 40 62 06
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-50
Send	Command: 84 A9 61 00 02 40 64 01
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-51
Send	Command: 84 A9 61 00 02 40 66 01
Pause 100
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-STEP3-52
Send	Command: 84 A9 61 00 02 40 68 39
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-STEP3-53
Send	Command: 84 A9 61 00 02 40 6B 39
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-STEP3-54
Send	Command: 84 A9 61 00 02 40 6C 39
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-STEP3-55
Send	Command: 84 A9 61 00 02 40 6F 39
Receive	Command:84 A9 61 00 02 40 17 00
Command ID:	WM-STEP3-42
Send	Command: 84 A9 61 00 02 40 54 00
Receive	Command:84 A9 61 00 02 40 17 00
