//Verison=2.0
//Example,Don't Delete flowing text, 下面是例子,请不要删除
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary:结束通话 // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '61 00 02 00 19 00' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//

Command ID:	FLASH_INITIAL
Send	Command: 84 A9 61 00 02 00 93 03
Receive	Command:84 A9 61 00 02 00 93 00
PAUSE 500
Command ID:	FLASH_HEAD
Send	Command: 84 A9 61 00 07 00 90 00 00 00 00 88 00 00
Receive	Command:84 A9 61 00 02 00 90 00
PAUSE 200
Command ID:	FLASH_DATA136
Send	Command: 84 A9 61 01 01 00 91 00 CF 00 CF FE 06 00 CF 00 CF 00 CF 00 CF 00 CF 7C 06 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 78 00 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF F4 03 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 44 05 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF BA 02 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF AB 02 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 60 05 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF FA 05 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 2E 03 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 8B 02 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 16 06 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 7B 02 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 73 02 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 6B 02 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 63 02 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00
Receive	Command:84 A9 61 00 02 00 91 00
PAUSE 500
Command ID:	RD_FLASH_DATAH
Send	Command: 84 A9 61 00 05 20 94 00 00 10 0A 00
Receive	Command:84 A9 61 00 0B 20 94 00 00 00 00 88 00 00 05 60 00
Command ID:	RD_FLASH_DATA
Send	Command: 84 A9 61 00 05 20 94 00 05 60 78 00
Receive	Command:84 A9 61 00 79 20 94 00 CF 00 CF FE 06 00 CF 00 CF 00 CF 00 CF 00 CF 7C 06 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 78 00 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF F4 03 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 44 05 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF BA 02 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF AB 02 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 00 CF 60 05 00 CF 00 CF 00 CF
Command ID:	FLASH_START
Send	Command: 84 A9 61 00 03 00 92 12 34 00
Receive	Command:84 A9 61 00 02 00 92 00
Command ID:	RD_FLASH_START
Send	Command: 84 A9 61 00 01 20 92 00
Receive	Command:84 A9 61 00 03 20 92 12 34
Command ID:	RD_FLASH_DATAS
Send	Command: 84 A9 61 00 05 20 94 00 00 00 10 00
Receive	Command:84 A9 61 00 11 20 94 FF FF FF FF FF FF FF FF 12 34 FF FF FF FF FF FF
Command ID:	FLASH_END
Send	Command: 84 A9 61 00 02 00 93 00
Receive	Command:84 A9 61 00 02 00 93 00
Command ID:	FLASH_HEAD
Send	Command: 84 A9 61 00 07 00 90 00 00 00 00 88 00 00
Receive	Command:84 A9 61 00 02 00 17 06
Command ID:	FLASH_INITIAL
Send	Command: 84 A9 61 00 02 00 93 03
Receive	Command:84 A9 61 00 02 00 93 00
Command ID:	RD_FLASH_DATA
Send	Command: 84 A9 61 00 05 20 94 00 05 60 78 00
Receive	Command:84 A9 61 00 79 20 94 FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF
Command ID:	RD_FLASH_ID
Send	Command: 84 A9 61 00 01 20 90 00
Receive	Command:84 A9 61 00 0B 20 90 BF 8C BF 8C BF 8C BF 8C BF 8C
Command ID:	FLASH_END
Send	Command: 84 A9 61 00 02 00 93 00
Receive	Command:84 A9 61 00 02 00 93 00
