//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//


.Set READY_VAR = 01
Command ID: WORK_MODE_DUPLEX
Send command: 84 A9 61 00 04 00 18 03 00 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: PROCESS_MODE
Send command: 84 A9 61 00 02 00 1A 03
Receive Data: 84 A9 61 00 02 00 1A 00
Command ID:	DMR_FLC
Send	Command: 84 A9 61 00 04 05 76 05 05 05
Receive	Data:84 A9 61 00 02 05 76 00
Command ID:	DPMR_CC
Send	Command: 84 A9 61 00 02 05 77 0d
Receive	Command:84 A9 61 00 02 05 77 00

Command ID: DPMR_CALLED_ID_BCD
Send command: 84 A9 61 00 05 03 7D 01 23 45 67
Receive Data: 84 A9 61 00 02 03 7D 00
Command ID: DPMR_OWN_ID_BCD
Send command: 84 A9 61 00 05 03 7E 01 23 45 67
Receive Data: 84 A9 61 00 02 03 7E 00
Command ID:	REPORT_FIELD
Send	Command: 84 A9 61 00 02 00 1D Ff
Receive	Command:84 A9 61 00 02 00 1D 00
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
PAUSE 500
Receive	Data:84 A9 61 00 02 05 78 00
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B D1
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 12 D6 87
Receive	Data:84 A9 61 00 04 30 51 12 D6 87
Receive	Data:84 A9 61 00 05 30 7D 01 23 45 67
Receive	Data:84 A9 61 00 05 30 7E 01 23 45 67
Receive	Data:84 A9 61 00 02 30 27 00
Pause 1200
Command ID:	DPMR_SEND_END
Send	Command: 84 A9 61 00 01 03 21 00
Receive	Command:84 A9 61 00 02 03 21 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B d2
Receive	Data:84 A9 61 00 01 30 4B
Receive	Command:84 A9 61 00 02 20 17 0A
//Receive	Data:84 A9 61 00 02 30 1B 08
Pause 500
Command ID: DPMR_OWN_ID_BCD
Send command: 84 A9 61 00 05 03 7E 02 44 56 70
Receive Data: 84 A9 61 00 02 03 7E 00
Command ID: DPMR_CALLED_ID_BCD
Send command: 84 A9 61 00 05 03 7D 01 22 56 70
Receive Data: 84 A9 61 00 02 03 7D 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Data:84 A9 61 00 02 00 19 00
Command ID: DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78 00
Receive	Data:84 A9 61 00 02 05 78 00
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 02 30 1B 04
Receive	Data:84 A9 61 00 02 30 7B D1
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 04 30 50 12 B3 C6
Receive	Data:84 A9 61 00 04 30 51 25 51 66
Receive	Data:84 A9 61 00 05 30 7D 01 22 56 70
Receive	Data:84 A9 61 00 05 30 7E 02 44 56 70
Receive	Data:84 A9 61 00 02 30 27  05
Pause 2000

Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Pause 500
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Data:84 A9 61 00 02 20 17 0A
Command ID:	REPORT_FIELD
Send	Command: 84 A9 61 00 02 00 1D 62
Receive	Command:84 A9 61 00 02 00 1D 00
Command ID:	DPMR_OWN_ID_BCD
Send	Command: 84 A9 61 00 05 03 7E 12 34 56 70 
Receive	Command:84 A9 61 00 02 03 7E 00
Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 12 34 56 70 
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 00
Pause 1000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 61 01
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 62 02
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 63 03
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 64 04
Receive	Command:84 A9 61 00 02 05 36 00

Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 65 05
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 66 06
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 67 07
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 68 08
Receive	Command:84 A9 61 00 02 05 36 00

Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 69 09
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 11 0A
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 22 0B
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 33 0C
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 44 0D
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 55 0E
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	GROUP_ID
Send	Command: 84 A9 61 00 06 05 36 01 23 45 77 0F
Receive	Command:84 A9 61 00 02 05 36 00
Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 61
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 12
Pause 2000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500
Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 62
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 22
Pause 1000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500
Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 63
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 32
Pause 2000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500
Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 64
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 42
Pause 1000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500

Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 65
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 52
Pause 2000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500
Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 66
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 62
Pause 1000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500

Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 67
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 72
Pause 2000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500
Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 68
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 82
Pause 1000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500

Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 69
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 92
Pause 2000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500
Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 11
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 A2
Pause 1000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500

Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 22
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 B2
Pause 2000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500
Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 33
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 C2
Pause 1000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500

Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 44
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 D2
Pause 2000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500
Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 55
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500

Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 E2
Pause 1000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500

Command ID:	DPMR_CALLED_BCD
Send	Command: 84 A9 61 00 05 03 7D 01 23 45 77
Receive	Command:84 A9 61 00 02 03 7D 00
Command ID:	DMR_CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Data:84 A9 61 00 02 05 78 00
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 04 30 76 05 05 05
Receive	Data:84 A9 61 00 05 30 7E 12 34 56 70
Receive	Data:84 A9 61 00 02 30 27 F2
Pause 2000
Command ID:	CARRIER_LOSE&CALL_END
Send	Command: 84 A9 61 00 03 00 21 19 00 
Receive	Command:84 A9 61 00 02 00 19 00
Receive	Command:84 A9 61 00 02 20 17 0A

Pause 500